**Fish Sampling**

* Sampling Points
  + A grid of 50-meter spaced points will be selected as potential gillnet and electrofishing sites from the sampling area of Bluff Lake.
    - A subset of 5 points will be selected and randomly assigned each sampling period as gillnet or electrofishing sites.
  + Sites for fyke nets and minnow traps will be selected by following a randomly selected bearing from the midpoint of the sampling area to the bank.
  + Additional random sites will be selected for each gear for instances when nets or lines could not be deployed in the originally selected sites.
* Gear Setup
  + Fyke nets will be anchored to the bank and set perpendicular to shore.
  + Fyke nets and minnow traps will be left to soak overnight and checked each day of the sampling period.
  + Gillnets will be checked every 2-4 hours and pulled at the end of each sampling day.
* Fish handing
  + Target fish species will be identified and measured to the nearest millimeter.
  + Sportfish species over 150 mm will be weighed individually.